|  |  |
| --- | --- |
| Product | Hunter Douglas® Folding Shutter |
| System | Folding Shutter with perforated metal sheet |
| Material | Aluminium frame with aluminium perforated sheet on front |
| Perforations | * Z 2.5 x 10 mm (5% open) * Z 3.5 x 10 mm (10% open) * Custom perforation or pattern |
| Frame | Vertical: Aluminium 60 x 40 mm rectangular hollow profile Horizontal: Aluminium 60 x 80 mm extrusion box profile with snap-in cover |
| Sizes | Bay Height\_\_\_\_\_\_ (max. height depending on wind loads Bay Width\_\_\_\_\_\_ (max. width depending on wind loads)  Max panel height 3000 mm  Max panel width 900 mm, for motorized folding shutter minimum panel width 530 mm |
| Top rail | Aluminium extruded rectangular profile 40 x 48 mm |
| Bottom rail | Double aluminium extruded box profile 40 x 20 mm |
| Alloy extrusions | Al-Mg-Si 0.5 F22 (EN-AW 6060 T6/T66) |
| Accessories | Hunter Douglas® top runners, bottom runners and pivots in aluminium, plastic and stainless steel  Hinges in aluminium  Locking devices (manual operation) in stainless steel and aluminium |
| Fin fixing | With stainless steel fastening materials in A2 (304) quality |
| Finish | * Natural anodised 20 microns (VOM1/A20/VB6) (frame only) * Custom colour anodised (limited range) 20 microns (frame only) * Polyester powder coated to RAL or other industry standard colour, thickness 60 microns, gloss \_\_\_% (standard gloss 70%) * Polyester powder coated to RAL or other industry standard colour, thickness 90 microns, gloss \_\_\_% (standard gloss 70%)   Please note: perforated metal sheet always powdercoated |
| Rail fixation | Rail fixed to ceiling/ floor or façade by means of aluminium brackets |
| Motorization (optional) | Proprietary Hunter Douglas Flat Folding Shutter Drive system with 24V actuator.  Motor controller includes 230V transformer.  Optional: automated control system including wind protection |