|  |  |
| --- | --- |
| Product | Hunter Douglas® Sliding Shutter  |
| System | Perforated Sliding Shutter  |
| Material | Frameless cassette in aluminium sheet metal Al 99.5 |
| Perforations | * Z 2.5 x 10 mm (5% open)
* Z 3.5 x 10 mm (10% open)
* Custom perforation or pattern
 |
| Sizes | Shutter Height\_\_\_\_\_\_ (max. height depending on applicable wind loads)Shutter Width\_\_\_\_\_\_ (max. width depending on applicable wind loads)Shutter Depth 60 mm |
| Top rails | Aluminium extruded rectangular profile 40 x 48 mm |
| Bottom rails | * Aluminium extruded T-profile 50 x 40 mm
* Double aluminium extruded box profile 40 x 20 mm
 |
| Alloy extrusions | Al-Mg-Si 0.5 F22 (EN-AW 6060 T6/T66) |
| Accessories | Hunter Douglas® top runners, bottom runners and end stop |
| Fixing materials | Stainless steel A2 (304) quality |
| Finish | * Polyester powder coated to RAL or other industry standard colour, thickness 60 microns, gloss \_\_\_% (standard gloss 70%)
* Polyester powder coated to RAL or other industry standard colour, thickness 90 microns, gloss \_\_\_% (standard gloss 70%)
 |
| Rail fixation | Rail fixed to façade or floor by means of aluminium brackets  |
| Motorization | Optional: proprietary Hunter Douglas Sliding Shutter Drive system, 24V belt drive. Motor controller includes 230V transformer.* 1 / 2 / 3 / 4 shutters driven by one motor (max total shutter weight 120 kg)

Optional: automated control system |